# ID 70283

Drive error during zero pulse search.
Description | An error has occurred in the drive during the zero pulse search. Consult the documentation of the drive manufacturer for a further error diagnosis.
Response | Class | 7 | Closed-loop controlled axis stop
Solution | Class | 6 | Consult drive manufacturer's documentation
Parameter | %1: | Current value [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Drive type [-]
Drive type of concerned axis, see P-AXIS-00020
%3: | Block number [-]
Block number of the NC program, in which the error occurred.
Error type | 11, Error message from position controller.