# ID 110609

An invalid bit number was entered for the 'value_latched' signal.
Description | When configuring the SERCOS real-time status bits for the signal 'value latched probe 1/2', an invalid bit number was entered either in P-AXIS-00678 (probe 1) or in P-AXIS-00684 (probe 2).
Response | Class | 3 | An error message is output containing the axis parameters P-AXIS-00118 (measurement axis) and P-AXIS-00098 (kasto_achse) are reset in order to prevent the execution of measurement run or edge banding with incompletely configured probes.
Solution | Class | 1 | Correct P-AXIS-00678/or P-AXIS-00684.
Parameter | %1: |
Log. axis number
%2: |
Incorrect value of P-AXIS-00678/or P-AXIS-00684
%3: |
Permissible minimum value.
%4: |
Permissible maximum value.
Error type | 2, Error message on data transfer of parameter lists to controller.