# ID 110352

Axis mode not permitted for spindle.
Description | The axis mode P-AXIS-00015 is not set to MODULO (= 4) for the spindle , even though this is required. However, this is necessary for a spindle.
Response | Class | 1 | Value is set to MODULO
Solution | Class | 1 | Correct value in parameter list.
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [-]
P-AXIS-00015
%3: | Corrected value [-]
P-AXIS-00015
Error type | 2, Error message by data transfer from parameter list into control device.