# Parameters

Cycle parameters | Description
@P2 | Tool diameter
@P23 | Fine measurement repetitions
@P37 | Permissible tolerance of the measuring points.
@P64 | Mode 0 = push 1 = pull
@P66 | Length offset Only positive values are permissible. The point on the tool to be measured. Tool corner radius +0.5mm
@P67 | Radius offset Only positive values are permissible. Tool offset to generate a precise measurement. The value should stand at 0 for pointed tools, small tools and spherical tools. Tool radius – tool corner radius – 0.5mm