# ID 110545

Monitoring of homing movement distance is only for spindles and rotary axes possible.
Description | Parameter P-AXIS-00412 was set to a value other than zero (nil) although the axis does not have the axis type spindle or rotatory (see also P-AXIS-00018). Parameter P-AXIS-00412 can only be used together with spindles or rotary axes.
Response | Class | 3 | Warning output, P-AXIS-00412 is set to zero (nil).
Solution | Class | 1 |
Parameter | %1: | Logical axis number [-]
%2: | Error value [-]
Set value of P-AXIS-00412.
%3: | Corrected value [-]
Corrected value of P-AXIS-00412.
Error type | 2, Error message by data transfer from parameter list into control device.