# Configuration files

The SysCalibConfigLaser.nc file is executed before each cycle to calibrate the laser.

Variables | Description
V.CYC.LASER_POS_X | Position of the laser focal point in the X axis
V.CYC.LASER_POS_Y | Position of the laser focal point in the Y axis
V.CYC.LASER_POS_Z | Position of the laser focal point in the Z axis
V.CYC.DIRECTION | Definition of measuring and positioning direction: 0- Positioning takes place in X+ and measuring in X- direction 1- Positioning takes place in Y+ and measuring in Y- direction 2- Positioning takes place in X- measuring in X+ direction 3- Positioning takes place in Y- and measuring in Y+ direction
V.CYC.LASER_Z_START_POS | This position is approached before the first measurement in Z. It should be a couple of mm above the laser focal point.
V.CYC.LASER_Z_END_POS | This position is approached for the first measurement It should be a couple of mm under the laser focal point.

These 2 files control the activation and deactivation of the lasers:

1. SysCalibConfigLaserOn.nc
2. SysCalibConfigLaserOff.nc