# ID 70124

Defined master axis not configured as gantry master.
Description | The master axis for gantry mode specified in the axis parameters is not configured as a master axis. Solution: Parameterise axis as gantry master with logical axis number (P-AXIS-00015) See also FCT-C11// Section: Overview]
Response | Class | 1 | Warning
Solution | Class | 7 | Set the correct operation mode for the master axis
Parameter | %1: | Logical axis number [-]
Logical axis number of gantry slave axis, see P-AXIS-00016
%2: | Logical axis number [-]
Logical axis number of specified master axis, see P-AXIS-00016
Error type | -