# ID 50922

Radius not zero on start move.
Description | When the ORBIT channel is activated, the radius must be 0 (corresponds to the Y PCS position in the DR channel). This is not the case.
Response | Class | 4 | Movement stop.
Solution | Class | 7 | Before the ORBIT channel is activated, the radius (Y axis) must be programmed to 0 in the DR channel.
Parameter | %1: | Current value [0.1 10^-3 mm or ø]
Current radius (Y PCS position in the DR channel)
%2: | Limit value [0.1 10^-3 mm or ø]
Maximum permitted radius when the ORBIT channel is activated
Error type | 1, Error message from NC program.