# Number of bits for command value (P-AXIS-00816)

P-AXIS-00816 | Number of bits for command value
Description | This parameter limits the command value output by the position controller to the value range that can be used by the drive or terminal.
Parameter | kenngr.bit_range_comand_value
Data type | UNS16
Data range | 8…32
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 32
Drive types | Conventional, SERCOS, Terminal, Lightbus, Profidrive, CANopen, DSE
Remarks | Available as of CNC Build V3.1.3080.06