# ID 20676

Invalid angle.
Description | When programming the NC command #CS ON[...], an inadmissible rotation angle was programmed inside the square brackets. Syntax example: Wrong: #CS ON [10,20,0,45,0,450] Correct:

#CS ON [10,20,0,45,0,90]

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. In the NC command #CS ON[...] the rotation angles may only be programmed between -360° and +360°. For further information see [PROG// Section: Defining a machining coordinate system]
Parameter | %1: | Error value[0.1 µm or 0.0001°]
%2: | Lower limit value [-]
%3: | Upper limit value [-]
Error type | 1, Error message from NC program.