# ID 50573

Edge bending measurement cycle still active.
Description | The channel parameter P-CHAN-00153 at the edge bending controls whether the end of the measuring cycle or the SERCOS command S-0-170 is implicit or controlled via G107. In the event of an error, deactivation via G107 is missing at at program end.

For more information on edge bending see [PROG// Section: Edge bending].

Response | Class | 4 | Movement stop.
Solution | Class | 6 | Before program end or M30 execute, correct deselecting with G107
Error type | 1, Error message from NC program.