# ID 60131

Selection of feedrate in millimetre per revolution by stationary spindle.
Description | In the NC program, with the spindle stopped, the command G96 (feedrate per revolution) has been programmed.
Response | Class | 6 | Abort NC program.
Solution | Class | 6 | Before programming G96, program M3/M4 in the NC program.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
Error type | 1, Error message from NC program..