# ID 50884

Actual position request for axis moving to fixed stop not possible.
Description | While an axis is located at the fixed stop [FCT-M8] no actual position request may be made for this axis. The Move to fixed stop function was not deactivated during a preceding CNC reset since the axis is still located at the fixed stop. Example with error:

#CHANNEL INIT [ACTPOS] (* Error message 50884 *)

Possible solution:

G01 X0 F1000 X[FIXED_STOP OFF]

#CHANNEL INIT [ACTPOS]

Response | Class | 4 | Controlled halt of the axis, the control loop is closed.
Solution | Class | 6 | Check and modify the NC program. Ignore the affected axis in the actual position request.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Current value [-]
State of the Move to fixed stop function
%3: | Current value [-]
State of the fixed stop detection function
Error type | 1, Error message from NC program.