# ID 13167

Tool radius greater than corner radius.
Description | A check is made as to whether the programmed corner radius can be manufactured with the current milling cutter. In this case, the tool radius must be less than or at maximum equal to the corner radius. If not, the message is generated.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Use a tool with a radius less than or equal to the programmed corner radius for machining.
Error type | 1, Error message from the NC program