# Lower limit of security zone 1 (P-AXIS-00093)

P-AXIS-00093 | Lower limit of security zone 1
Description | This parameter defines the lower limit of security zone 1. The lower limit of the security zone must be smaller than the upper limit. P-AXIS-00093 < P-AXIS-00085 This position is limited by the software limit switches (P-AXIS-00177 and P-AXIS-00178).
Parameter | kenngr.red_speed_zone_neg
Data type | SGN32
Data range | P-AXIS-00177 < P-AXIS-00093 < P-AXIS-00178
Axis types | T, R
Dimension | T: 0.1µm | R: 0.0001°
Default value | 0
Drive types | ----
Remarks |