# ID 150099

Upper limit for handwheel increments may not be 0.
Description | The manual mode parameters are read and interpreted by the CNC. The program detects that the value 0 was specified in the manual mode parameters for one of the P-MANU-00007 parameters.
Response | Class | 3 | Manual mode parameters are not transferred to the CNC.
Solution | Class | 6 | Correct the value for P-MANU-00007 so that it is > 0. Reinterpret manual mode parameters by restarting CNC system.
Parameter | %1: | Current value [-]
Value specified in the manual mode parameter record for P-MANU-00007.
%2: | Limit value [-]
Limit value that was exceeded.
%3: | Logical identifier of control element [-]
Logical identifier of control element where the value of parameter P-MANU-00007 exceeds the limit value.
Error type | 2, Error message on data transfer of parameter lists to controller.