# D/A-channel number (P-AXIS-00048)

P-AXIS-00048 | D/A-channel number
Description | The parameter defines the D/A-channel number.
Parameter | lr_hw[i].da_channel
Data type | UNS32
Data range | 0 ≤ da_channel < depending on hardware
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Drive types | Conventional, Terminal, Lightbus, Profidrive
Remarks | This entry is not adopted when the axis parameter list is updated. Updates only become effective when the controller is rebooted.