# Parameters

@P37 | Permissible tolerance of the measuring points. Select a reasonable value here since it is only used for a check. It the tolerance is too small, it may result in unnecessary machine stops.
@P67 | Radius offset Only positive values are permissible. Tool offset to generate a precise measurement. Set the offset according to the tool measurement.

## Additional information

- Syntax
- Programming example