# ID 70655

Secondary encoder not found.
Description | A secondary encoder was configured in the axis parameter list using P-AXIS-00824. The configured entry was not found.
Response | Class | 1 | Warning output.
Solution | Class | 1 | Check and modify the entry for the secondary encoder P-AXIS-00824. The parameterised drive signal must match the data item of the parameterised nc_ref.
Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016) of master axis
%2: | Error value [-]
Secondary encoder signal P-AXIS-00824 that is to be used.
Error type | 11, Error message from position controller.