# ID 110571

Positive absolute ACS manual mode limit exceeds positive software limit switch.
Description | The absolute positive movement limit P-AXIS-00493 for the movement range in active manual operation mode is greater than the negative software limit switch P-AXIS-00178. The absolute positive movement limit is set to the positive software limit switch.
Response | Class | 1 | None.
Solution | Class | 1 | Set positive motion limit P-AXIS-00493 smaller than positive software limit switch.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current value for positive movement limit P-AXIS-00493.
%3: | Limit value [-]
Current value für positive software limit P-AXIS-00178.
%4: | Corrected value [-]
Corrected value for positive motion limit P-AXIS-00493.
Error type | 2, Error message by data transfer from parameter list into control device.