# Measure angle between point in X and drilled hole (C axis)

Position the touch probe in front of the required surface above the workpiece, either manually or in automatic mode, before the cycle is started.

If no C axis is configured, call the cycle without transferring @P7. The twist in C can be manually transferred to the related zero offset by evaluating the output variables in the post-program.

Measure angle between point in X and drilled hole (C axis)

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables