# ID 50529

Incorrect parameter setting for measurement run to fixed stop.
Description | In conjunction with the measurement function G100, several measurement types are available. These types can be selected via the MDS or the CNC program. An impermissible parameter setting is active during a measurement run to fixed stop. For detailed information on G100, see

- [FCT-C4],
- [PROG// Section: Measuring functions]
- [PROG// Section: Settings for measurement]

Response | Class | 4 | Movement stop.
Solution | Class | 6 | Change measurement type or parameter value 2
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis
%2: | Current value [-]
Name of machine data record parameter
%3: | Current value [-]
Machine parameter value
%4: | Current value [-]
Selected measurement type
%5: | Current value [-]
Measurement axes with motion
Error type | 1, Error message from NC program..