# ID 20545

An axis involved in synchronous operation can not be released.
Description | An axis programmed in the axis exchange command is currently used in synchronous operation mode and must not be released. Example: Wrong: N30 #SET AX LINK[1, B=X] N40 #ENABLE AX LINK[1]

:

N70 #PUT AX[X]

:

N80 #DISABLE AX LINK[1]

:

N1000 M30

Correct:

N30 #SET AX LINK[1, B=X]

N40 #ENABLE AX LINK[1]

:

N70 #DISABLE AX LINK[1]

:

N80 #PUT AX[X]

:

N1000 M30

For further information see [PROG// Section: Synchronous operation]

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the program flow sequence. Before the axis exchange command, the synchronous operation must be deselected.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
%3: | Current value [-]
Error type | 1, Error message from NC program.