# ID 21304

Channel parameters: SLOPE parameter exceeds permissible value range.
Description | One of the default slope parameters specified in the channel parameters (P-CHAN-00071, P-CHAN-00073, P-CHAN-00001) exceeds the permissible number range.
Response | Class | 1 | Start-up of the control is continued.
Solution | Class | 1 | Check and modify the corresponding default slope parameter in the channel parameters before the next controller start-up. During start-up, in case of conflict, the invalid default slope parameter is set to zero (nil), and the start-up is continued.
Parameter | %1: | Error value [-]
%2: | Lower limit value [-]
%3: | Upper limit value [-]
%4: | Corrected value [-]
Error type | 2, Error message by data transfer from parameter list into control device.