# ID 70386

Usage of DC brake is only for spindles possible.
Description | Parameter P-AXIS-00410 was set to a value not equal to –1 (DC brake control was enabled), although the axis is not a spindle.
Response | Class | 1 | Warning output, P-AXIS-00410 is set to –1.
Solution | Class | 1 | The use of a DC brake is only possible for spindles. Deactivate DC brake by setting P-AXIS-00410 to -1.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Configured axis type, see P-AXIS-00018.
%3: | Error value [-]
Configured value of P-AXIS-00410.
%4: | Corrected value [-]
Corrected value of P-AXIS-00410.
Error type | 2, Error message by data transfer from parameter list into control device.