# ID 120711

Lift and synchronisation movements with active HSC slope not possible.
Description | When a lift movement is programmed with the function “Advanced lifting”, it is not permitted to use the HSC slope.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the NC program. Change the slope type, e.g. #SLOPE [ TYPE=STEP]
Error type | 1, Error message from NC program.