# ID 110062

Modification of the logical axis number requires restart of the control.
Description | The parameter P-AXIS-00016 for unique identification of an axis in the system cannot be changed while the CNC kernel is running. The new logical axis number is not transferred; the previous active logical axis number remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Only change the logical axis number P-AXIS-00016 in configuration mode or when the CNC is not running.
Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016
%2: | Current value [-]
Current value of P-AXIS-00016.
%3: | Corrected value [-]
Corrected value of P-AXIS-00016.
Error type | 2, Error message on data transfer of parameter lists to controller.