# ID 120542

Parameter change during active b-spline interpolation not possible.
Description | An attempt was made to change the parameterization when B-spline path smoothing was active. (e.g. #HSC [BSPLINE TRACK_DEV=5 MERGE=0 AUTO_OFF_PATH=1]). Please turn off B-spline before parameters are changed.
Response | Class | 1 | The new value of the parameter is dismissed
Solution | Class | 1 | Change of NC-program
Parameter | %1: | NC block number [-]
Block number of parameter change
%2: | Current value [-]
Parameter type: 0x0040 PATH_DEV 0x0080 TRACK_DEV 0x0100 MAX_PATH_LENGTH 0x0200 MAX_ANGLE
0x0400 AUTO_OFF_G00
0x0800 MERGE_DEV
0x1000 MERGE_RETRY
0x2000 MERGE_WINDOW
0x4000 PATH_SPLIT bzw AUTO_OFF_PATH

0x8000 TRACK_SPLIT bzw AUTO_OFF_TRACK

0x10000 LIMIT_CORNER_DIST

%3: | Current value [-]
Current parameter value
%4: | Error value [-]
Wanted, new value of parameter
Error type | 1, Error message from NC program.