# ID 70432

Parametrized greatest index of cross compensation table exceeds limits.
Description | In the compensation value list, parameter P-COMP-00004 for cross compensation specifies the value (starting with 0) of the index of the last valid entry in the compensation value list for cross compensation. During interpretation of that list by the CNC it is checked if the specified index is between the limits that are provided for cross compensation.

See [COMP// Section: Cross compensation]

Response | Class | 7 | Closed-Loop controlled stop of axis, the cross compensation is turned off.
Solution | Class | 7 | Check the value in parameter P-COMP-00004 The value must be within the specified limits of the error message.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned slave axis
%2: | Error value [-]
Value specified by the operator in parameter P-COMP-00004 for the index of the last valid entry in the compensation value list for cross compensation.
%3: | Lower limit value [-]
Under limit value, P-COMP-00004 must be greater than or equal to this value.
%4: | Upper limit value [-]
Upper limit value, P-COMP-00004 must be less than or equal to this value.
Error type | 2, Error message by data transfer from parameter list into control device.