# ID 70402

Setting/resetting of bits with #DRIVE command is not supported for this communication type.
Description | In axis parameter P-AXIS-00399, 'BITARRAY_16' or 'BITARRAY_32' was configured as data type, although bitwise writing of drive values is not supported for the communication type configured in P-AXIS-00397. See also: [PROG// Section: Drive-independent switching of drive functions
Response | Class | 7 | Error message output, evaluation of drive functions is aborted.
Solution | Class | 6 | Customise either P-AXIS-00399 or P-AXIS-00397.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Name of the configured drive function (P-AXIS-00396).
%3: | Drive type [-]
Drive type (P-AXIS-00020).
%4: | Error value [-]
Configured communication type (P-AXIS-00397).
%5: | Error value [-]
Configured data type (P-AXIS-00399).
Error type | -