# ID 120742

Independent axis movement not permitted for axes belonging to an active work or protection area.
Description | Axes belonging to an active workspace or protection area may not be moved by an independent axis movement (see FCT-C14). This also includes lift movements. For further information see:

- For programming: [PROG// Section: Definition of a control area]
- For lift movements: [FCT-A11//Section: Overview]

Example:

#CONTROL AREA BEGIN [ID1 PROT POLY MIN_EXCUR=0 MAX_EXCUR=360]

G01 F1000 G90

X = 0 Y = 0

X = 0 Y = 100

X = 100 Y = 100

X = 100 Y = 0

X = 0 Y = 0

#CONTROL AREA END

#CONTROL ARA ON [ID1]

X[INDP_ASYN G0 G90 POS150] (Error 120742)

Response | Class | 2 | Error message output and NC program abort
Solution | Class | 6 | Correct NC program
Parameter | %1: | Current value [-]
ID of affected workspace or protection space
%2: | Current value [-]
For actual control area relevant axes
%3: | Error value [-]
Currently axis moving independently
Error type | 1, Error message from NC program.