# ID 90057

Adapting of feed rate impossible within G05 (tool radius exceeds range).
Description | The feedrate cannot be adapted with G11 when tool radius compensation is selected or deselected with G05. The tool radius is too large for this.
Response | Class | 1 | NC program processing is continued
Solution | Class | 1 | Use a tool with a smaller radius
Parameter | %1: | Current value [0.1 µm or 0.0001°]
Tool radius
%2: | Current value [0.1 µm or 0.0001°]
Theoretical radius of the tangential determined path
%3: | Current value [0.1 µm or 0.0001°]
Corrected radius of the tangential path
%4: | Lower limit value [0.1 µm or 0.0001°]
Error type | 1, Error message from NC program.