# Maximum number of segmented blocks for feed profile planning (P-CHAN-00375)

P-CHAN-00375 | Maximum number of segmented blocks for feed profile planning (HSC)
Description | To avoid unnecessarily small feed values, motion blocks are segmented. This parameter defines the maximum number of additional blocks generated by segmentation.
Parameter | hsc.gen.slope_segmentation_nbr_blocks
Data type | UNS32
Data range | 0 < slope_segmentation_nbr_blocks < MAX(UNS32)
Dimension | ----
Default value | 100
Remarks | The default value may only be changed after approval by the controller manufacturer.