# ID 310022

Axis was released with active distance control.
Description | When axis-specific distance control is active, one or several axes are to be released and their distance controlled. This is not permitted.
Response | Class | 7 | Controlled halt of the axis, the control loop is closed.
Solution | Class | 6 | Check and modify the process. Release the axis after deselecting distance control
Parameter | %1: | Logical axis number [-] or Logical channel number [-]
Logical axis number Axis parameters of the axis affected for axis-specific distance control, logical channel number Logical number of a NC channel (P-CHAN-00400) for 3D distance control.
%2: | Block number [-]
Block number in the NC program
%3: | Error value [0.1 10^-7 mm or ø]
Current offset due to distance control
%4: | Current value [-]
Current state of distance control
Error type | -