# ID 150088

Number of hand wheels does not coincide number of logical hand wheels.
Description | When interpreting manual mode parameter, it is detected that there are more or less handwheel parameter sets than determined by parameter P-MANU-00001 .
Response | Class | 3 | Manual mode parameters aren’t taken over into CNC, but CNC start-up is continued using default parameters.
Solution | Class | 6 | Correct value for parameter P-MANU-00001 or Add missing/remove surplus handwheel parameter data sets.
Parameter | %1: | Current value [-]
Value of parameter P-MANU-00001 from manual operation parameter data set.
%2: | Expected value [-]
During interpretation of manual mode parameters, handwheel parameter sets were found.
Error type | 2, Error message by data transfer from parameter list into control device.