# ID 110523

Software limit switch was adjusted because of resolution settings.
Description | The positive software limit switch P-AXIS-00178 or the negative software limit switch P-AXIS-00177 is out of range. This range is defined by the distance resolution of the measurement system.
Response | Class | 1 | Initialise the software limit switch
Solution | Class | 1 | Correct software limit switch in parameter list
Parameter | %1: | Logical axis number [-]
Log. axis number P-AXIS-00016
%2: | Incorrect value [-]
Software limit switches P-AXIS-00177/P-AXIS-00178
%3: | Current value [-]
Numerator of distance resolution P-AXIS-00234.
%4: | Current value [-]
Denominator of the distance resolution P-AXIS-00233.
%5: | Corrected value [-]
Corrected value of software limit switch.
Error type | 2, Error message on data transfer of parameter lists to controller.