# Weighting factor for rapid feed velocity (P-AXIS-00433)

P-AXIS-00433 | Weighting factor for rapid feed velocity (dynamic weighting)
Description | This parameter defines the weighting factor for rapid traverse velocity in the i element.
Parameter | dynamic_weighting.param[i].velocity_fact
Data type | UNS32
Data range | 10 < velocity_fact < MAX(UNS32)
Axis types | T, R
Dimension | T: 0.1% | R: 0.1%
Default value | 0
Drive types | ----
Remarks |