# ID 20765

Double-programmed M-function.
Description | In the NC block, an M function (techno function) with the same number is programmed several times channel-specifically, axis-specifically or spindle-specifically. Example for inadmissible double programming: N10 G00 X10 M10 M10 (channel-specific technofct.)

N10 G00 X10 X[M10] X[M10]] (axis-specific technofct.)

N10 G00 X10 S[M10 M10] (spindle-specific technofct.)

:

Example for allowed programming:

N10 G00 X10 M10 X[M10] S[M10] (combined technofct.)

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the programming of the M functions in the NC block. Remove surplus channel specific, axis specific or spindle specific M functions.
Parameter | %1: | Current value [-]
Number of the multiple programmed M function
Error type | 1, Error message from NC program.