# ID 20893

#CAX OFF not allowed during active transformation.
Description | Deselection of the C axis with the command #CAX OFF is not permitted when the transformation is active. Example with error: N100 #CAX N110 #CYL [Z, C, X60] N120 G00 G90 Z0 C0

N130 G01 C100 F500

N140 G02 Z100 R50

N150 #CAX OFF

N160 G01 C0

N170 Z0

N180 #CYL OFF

Corrected example:

N100 #CAX

N110 #CYL [Z, C, X60]

N110 G00 G90 Z0 C0

N130 G01 C100 F500

N140 G02 Z100 R50

N150 G01 C0

N160 Z0

N170 #CYL OFF

N180 #CAX OFF

[PROG// Section: Exchanging spindles in coordinated motion]

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Before deselection of the C-axis (#CAX OFF) the active transformation (#CYL OFF, #FACE OFF) has to be deselected in the NC program.
Error type | 1, Error message from NC program.