# ID 21579

Invalid setting of H-function by tube profile parameter.
Description | The parameter setting of active function tube profile machining #CYL[] contains invalid setting of M/H code number. Either the M/H code exceeds maximum permissible value or an internal locked M-code number was used (e.g. M30 program end mark).

Invalid parameter setting leads to deactivation of specific M/H-Code output.

Response | Class | 1 | Abort NC program processing.
Solution | Class | 1 | Check and correct parameter settings of channel machine data tube_profile.techno_nr_rnd_on, tube_profile.techno_nr_rnd_off
Parameter | %1: | Current value [-]
Current invalid M/H number
%2: | Limit value [-]
Maximum permissible M/H code number
%3: | Corrected value [-]
Corrected M/H-code number
Error type | 2, Error message by data transfer from parameter list into control device.