# Acceleration during position correction (P-AXIS-00366)

P-AXIS-00366 | Acceleration during position correction
Description | The parameter defines the effective acceleration of manual operation mode during use in a position correction.
Parameter | handbetrieb.ipo.hb_a_max_track
Data type | UNS32
Data range | 0 < hb_a_max_track ≤ 100000000 (Presetting of maximum axis acceleration, plausibility limit, application-specific)
Axis types | T, R, S
Dimension | T: mm/s² | R,S: °/s²
Default value | 0
Drive types | ----
Remarks | There is no limitation of the parameter values on the permissible maximum velocities P-AXIS-00212 and acceleration parameters P-AXIS-00008.