# ID 70256

Number of cycles for smooth coupling/decoupling of plane compensation too large.
Description | The filter cycles specified for plane compensation in the compensation value list to activate the compensation value across several position controller time cycles (see P-COMP-00027) is greater than the maximum permissible number. It is reduced to the maximum permissible value.

See:

[COMP// Section: Plane compensation]

[FCT-C5// Section: Plane compensation]

Response | Class | 1 | Warning, reduction of filter cycles to maximum permissible value.
Solution | Class | 1 | Reduce number of filter cycles in compensation value list see P-COMP-00027
Parameter | %1: | Logical axis number [-]
Logical axis number of the affected slave axis see P-AXIS-00016
%2: | Current value [-]
Number of specified filter cycles see P-COMP-00027
%3: | Corrected value [-]
Maximum permissible number of filter cycles
%4: | Block number [-]
Block number in the NC program at which the error occurred.
Error type | 2, Error message by data transfer from parameter list into control device.