# ID 20886

None of the programmed axes has axis mode C-axis.
Description | When face or lateral surface machining with the command #FACE or #CYL, the axes programmed in the command are not configured for C axis mode. In this case, the cause may be an incorrectly configured axis type or an incorrect axis mode in the associated axis parameter lists.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check the configured axes in the command for their axis type P-AXIS-00018 and axis mode P-AXIS-00015 . Note: A C axis must be configured as follows: kenngr.achs_typ 0x0002 or 0x0004 kenngr.achs_mode 0x0204
Error type | 1, Error message from NC program.