# ID 294505

KPS: Over voltage PMx.
Description | Intermediate circuit voltage is too high. Possible causes are: Defective ballast resistor. Ballast fuse.
Response | Class | 7 | Maximum braking. All active commands inhibited.
Solution | Class | 6 | Eliminate error. Reset by pressing the hardware acknowledgement button "ACK" on the front control panel.
Error type | 11, Error message from position controller.