# Consideration of distance control in software limit switch monitoring (P-AXIS-00428)

P-AXIS-00428 | Consideration of distance control in software limit switch monitoring
Description | This parameter defines whether the calculated distance control offset is included in the software limit switch monitor (see [FCT-A2]).
Parameter | kenngr.distc.check_sw_limit_switch
Data type | BOOLEAN
Data range | 0: Offset of distance control is not considered in software limit switch monitoring (Standard). 1: Offset of distance control is considered in software limit switch monitoring.
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
drive types. | SERCOS, Profidrive, CANopen
Remarks |