# ID 140053

Multiple use of same SERCOS drive address (configuration error).
Description | In the configuration data, two SERCOS axes are configured with the same drive address.
Response | Class | 3 | Error message output, but nevertheless the operation is continued.
Solution | Class | 6 | Check drive address in the configuration data.
Parameter | %1: | Logical axis number [-]
Logical axis number of first axis P-AXIS-00016).
%2: | Current value [-]
Drive address of first axis (P-AXIS-00019).
%3: | Logical axis number [-]
Logical axis number of second axis P-AXIS-00016).
%4: | Current value [-]
Drive address of second axis (P-AXIS-00019).
Error type | -