# Position of the second adaptation axis with acceleration test (P-COMP-00086)

P-COMP-00086 | Position of the second adaptation axis with acceleration test
Description | This parameter specifies the position of the second adaptation axis for the ith acceleration test.
Parameter | kw.crosstalk.position[i].ax_2
Data type | SGN64
Data range | MIN(SGN64) ≤ P-COMP-00086 < MAX(SGN64)
Axis types | T
Dimension | T: [0.1 µm] | R, S: -
Default value | 0
Remarks | Parameter available as of V3.1.3081.2 and V3.1.3108.4