# ID 110476

Compensation value change in leadscrew error compensation exceeds range of values.
Description | The difference between successive compensation values (see P-COMP-00023, P-COMP-00024) in the compensation value list for leadscrew error compensation is greater than permissible. If metric input in 0.1 µm is used (see P-COMP-00017), the compensation values in the controller are multiplied by the resolution of the axis (see P-AXIS-00234/P-AXIS-00233).
Response | Class | 3 | Leadscrew error compensation is not activated.
Solution | Class | 7 | Correct the compensation value list of the leadscrew error compensation. Reduce the distance between interpolation points (see P-COMP-00018) or insert additional interim points in the compensation value list to reduce the compensation value change per interval
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected
%2: | Current value [-]
Array index of the affected compensation value in the compensation value list
%3: | Current value [increments]
Current compensation value in increments (see P-COMP-00023/P-COMP-00024))
%4: | Current value [increments]
Current compensation value in increments (see P-COMP-00023/P-COMP-00024))
%5: | Incorrect value [increments]
Difference between both compensation values in increments
Error type | -