# ID 13433

Positioning feed rate must be higher than the measuring feed.
Description | The positioning feed rate V.P.Sys_Probes_feed_max must be greater than or equal to the measuring feed V.P.Sys_Probes_feed.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Change the feed values V.P.Sys_Probes_feed_max and V.P.Sys_Probes_feed in the NC program SysMeasWcsConfig.nc.
Error type | 1, Error message from the NC program