# Velocity during position correction (P-AXIS-00365)

P-AXIS-00365 | Velocity during position correction
Description | The parameter defines the effective velocity of manual operation mode during the use in a position correction.
Parameter | handbetrieb.ipo.hb_v_max_track
Data type | UNS32
Data range | 0 < hb_v_max_track ≤ 2000000000 (Presetting of maximum axis velocity, plausibility limit, application-specific)
Axis types | T, R, S
Dimension | T: µm/s | R,S: 0,001°/s
Default value | 0
Drive types | ----
Remarks |